# Copyright (C) 2010 The Android Open Source Project
#
# Licensed under the Apache License, Version 2.0 (the "License");
# you may not use this file except in compliance with the License.
# You may obtain a copy of the License at
#
#      http://www.apache.org/licenses/LICENSE-2.0
#
# Unless required by applicable law or agreed to in writing, software
# distributed under the License is distributed on an "AS IS" BASIS,
# WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
# See the License for the specific language governing permissions and
# limitations under the License.

#
# Input Device Calibration File for the Leo touch screen.
#

# Basic Parameters
touch.deviceType = touchScreen
touch.orientationAware = 1

# Size
touch.size.calibration = diameter
touch.size.scale = 10
touch.size.bias = 0
touch.size.isSummed = 0

# Pressure
# Driver reports signal strength as pressure.
#
# A normal thumb touch while touching the back of the device
# typically registers about 100 signal strength units although
# this value is highly variable and is sensitive to contact area,
# manner of contact and environmental conditions.  We set the
# scale so that a normal touch with good signal strength will be
# reported as having a pressure somewhere in the vicinity of 1.0,
# a featherlight touch will be below 1.0 and a heavy or large touch
# will be above 1.0.  We don't expect these values to be accurate.
touch.pressure.calibration = amplitude
touch.pressure.scale = 0.005

# Orientation
touch.orientation.calibration = none

